LIN

1. LIN version 2.0
2. Baud rate 19.2kbps
3. slaves node 4
4. master node 1
5. 13 Message
6. 4 types Message:response, ID, command slave y command all.
7. Signal types 5
8. Signal number 21
9. Signal endianess Little

???

* Toggle time
* Logical type (active low or active high)
* LED (on- board or extern)
* Scheduling table Ticks